tree de380dae6434868f1f3142d6225f23623d67963d
parent 12fe939f1df9482d6134f9ec5ae39ddacc3df426
author Tiwei Bie <tiwei.bie@intel.com> 1527180591 +0800
committer Michael S. Tsirkin <mst@redhat.com> 1528397751 +0300

content: support SR-IOV

Allocate a feature bit for virtio devices which support SR-IOV.
Note: at proposer's request, driver requirements have been
omitted - a reworked version is now being discussed.

Suggested-by: Michael S. Tsirkin <mst@redhat.com>
Signed-off-by: Tiwei Bie <tiwei.bie@intel.com>
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/11
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Acked-by: Cornelia Huck <cohuck@redhat.com>
